<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<hole x="13" y="106" drill="3.2"/>
<hole x="171" y="106" drill="3.2"/>
<text>1</text>
<text>1</text>
<text>3</text>
<text>5</text>
<text>2</text>
<text>4</text>
<text>6</text>
<text>1</text>
<text>12</text>
<text>23</text>
<text>34</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>5</text>
<text>4</text>
<text>6</text>
<text>8</text>
<text>10</text>
<text>7</text>
<text>9</text>
<text>JTAG</text>
<text>ISP</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>5V</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>!Step-ENB</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>!RESET</text>
<text>!SLEEP</text>
<text>STEP</text>
<text>DIRECTION</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>5V</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>!Step-ENB</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>!RESET</text>
<text>!SLEEP</text>
<text>STEP</text>
<text>DIRECTION</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>5V</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>!Step-ENB</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>!RESET</text>
<text>!SLEEP</text>
<text>STEP</text>
<text>DIRECTION</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>5V</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>!Step-ENB</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>!RESET</text>
<text>!SLEEP</text>
<text>STEP</text>
<text>DIRECTION</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>5V</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>!Step-ENB</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>!RESET</text>
<text>!SLEEP</text>
<text>STEP</text>
<text>DIRECTION</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>MS1</text>
<text>MS2</text>
<text>MS3</text>
<text>12V...25V</text>
<text>GND</text>
<text>GND</text>
<text>Power Supply</text>
<text>High current!!</text>
<text>use twin wiring</text>
<text>ATX</text>
<text>12V</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>12V</text>
<text>Switch</text>
<text>800mA</text>
<text>out</text>
<text>HeatBed</text>
<text>HotEnd0</text>
<text>1</text>
<text>2</text>
<text>HotEnd1</text>
<text>E0-Motor</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>E1-Motor</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>X-Motor</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>Y-Motor</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>Z-Motor</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>Z-Motor</text>
<text>2B</text>
<text>2A</text>
<text>1A</text>
<text>1B</text>
<text>GND</text>
<text>OUT</text>
<text>+5V</text>
<text>GND</text>
<text>OUT</text>
<text>+5V</text>
<text>GND</text>
<text>OUT</text>
<text>+5V</text>
<text>X-Endstop</text>
<text>Y-Endstop</text>
<text>Z-Endstop</text>
<text>-</text>
<text>+</text>
<text>Stepper</text>
<text>cooling fan
5V max. 100mA</text>
<text>n.c.</text>
<text>Heatbed</text>
<text>GND</text>
<text>Sens.</text>
<text>Sensor</text>
<text>Hotend1</text>
<text>GND</text>
<text>Sens.</text>
<text>Sensor</text>
<text>Hotend0</text>
<text>GND</text>
<text>Sens.</text>
<text>Sensor</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>+12V</text>
<text>max.500mA</text>
<text>100mA</text>
<text>5V</text>
<text>c</text>
<text>c</text>
<text>c</text>
<text>c</text>
<text>c</text>
<text>c</text>
<text>c</text>
<text>c</text>
<text>Hotbed</text>
<text>Hotend0</text>
<text>Hotend1</text>
<text>Fan(switch)</text>
<text>TxD</text>
<text>RxD</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>C</text>
<text>C</text>
<text>+</text>
<text>C</text>
<text>C</text>
<text>3,2mm</text>
<text>3,2mm</text>
<text>electronics easy</text>
<text>RepRap Controller dual Extruder</text>
<text>V2.0  20130410_DE</text>
<text>TOP</text>
<text>BOT</text>
<text>1</text>
<text>c</text>
<text>Stepper</text>
<text>Fan</text>
<text>GND</text>
<text>+5V</text>
<text>NC</text>
<text>RESET</text>
<text>µSD-Card</text>
<text>USB</text>
<text>RESET</text>
<text>µSD-Card</text>
<text>µUSB</text>
<text>GND</text>
<text>max.</text>
<text>Stepper Enable</text>
<text>Caution!! Sum of all 12V load currents
 must not exceed 1.3A and all 5V load
currents must not exceed 200mA.</text>
<text>1</text>
<text>+3,3V</text>
<text>+5V</text>
<text>+</text>
<text>-</text>
<text>Backlight</text>
<text>1</text>
<text>2</text>
<hole x="142" y="79.5" drill="3.2"/>
<hole x="65" y="56.5" drill="3.2"/>
<text>LCD-Connector</text>
<text>LCD-</text>
<text>C101</text>
<text>C102</text>
<text>C103</text>
<text>C104</text>
<text>C105</text>
<text>C106</text>
<text>C107</text>
<text>C108</text>
<text>C109</text>
<text>C110</text>
<text>C201</text>
<text>C202</text>
<text>C203</text>
<text>C204</text>
<text>C205</text>
<text>C206</text>
<text>C207</text>
<text>C208</text>
<text>C209</text>
<text>C210</text>
<text>C211</text>
<text>C212</text>
<text>C213</text>
<text>C214</text>
<text>C215</text>
<text>C216</text>
<text>C217</text>
<text>C218</text>
<text>C219</text>
<text>C220</text>
<text>C301</text>
<text>C302</text>
<text>C303</text>
<text>C304</text>
<text>C305</text>
<text>C306</text>
<text>C401</text>
<text>C402</text>
<text>C404</text>
<text>C405</text>
<text>C406</text>
<text>C407</text>
<text>C408</text>
<text>C409</text>
<text>C411</text>
<text>C412</text>
<text>C413</text>
<text>C414</text>
<text>C416</text>
<text>C417</text>
<text>C420</text>
<text>C421</text>
<text>C422</text>
<text>C423</text>
<text>C424</text>
<text>C425</text>
<text>C426</text>
<text>C501</text>
<text>C502</text>
<text>C503</text>
<text>C504</text>
<text>C601</text>
<text>C602</text>
<text>C603</text>
<text>C604</text>
<text>C605</text>
<text>C606</text>
<text>C607</text>
<text>C608</text>
<text>C609</text>
<text>C610</text>
<text>C611</text>
<text>C612</text>
<text>C613</text>
<text>D501</text>
<text>D502</text>
<text>D503</text>
<text>D504</text>
<text>D601</text>
<text>D602</text>
<text>D604</text>
<text>IC101</text>
<text>IC401</text>
<text>IC402</text>
<text>IC403</text>
<text>IC404</text>
<text>IC601</text>
<text>IC602</text>
<text>JP101</text>
<text>JP102</text>
<text>JP201</text>
<text>JP202</text>
<text>JP203</text>
<text>JP208</text>
<text>JP209</text>
<text>L601</text>
<text>L602</text>
<text>LCD401</text>
<text>LED101</text>
<text>LED401</text>
<text>LED402</text>
<text>LED403</text>
<text>LED501</text>
<text>LED502</text>
<text>LED503</text>
<text>LED504</text>
<text>LED602</text>
<text>R101</text>
<text>R102</text>
<text>R103</text>
<text>R104</text>
<text>R201</text>
<text>R202</text>
<text>R203</text>
<text>R204</text>
<text>R205</text>
<text>R301</text>
<text>R302</text>
<text>R303</text>
<text>R304</text>
<text>R305</text>
<text>R306</text>
<text>R401</text>
<text>R402</text>
<text>R403</text>
<text>R404</text>
<text>R405</text>
<text>R406</text>
<text>R407</text>
<text>R408</text>
<text>R409</text>
<text>R410</text>
<text>R411</text>
<text>R412</text>
<text>R501</text>
<text>R502</text>
<text>R503</text>
<text>R504</text>
<text>R505</text>
<text>R506</text>
<text>R507</text>
<text>R508</text>
<text>R509</text>
<text>R510</text>
<text>R511</text>
<text>R512</text>
<text>R513</text>
<text>R514</text>
<text>R515</text>
<text>R516</text>
<text>R517</text>
<text>R518</text>
<text>R601</text>
<text>R603</text>
<text>R604</text>
<text>R606</text>
<text>SW101</text>
<text>SW401</text>
<text>T101</text>
<text>T501</text>
<text>T502</text>
<text>T503</text>
<text>T504</text>
<text>T505</text>
<text>X201</text>
<text>X202</text>
<text>X203</text>
<text>X204</text>
<text>X205</text>
<text>X401</text>
<text>X402</text>
<text>X403</text>
<text>X404</text>
<text>X601</text>
<text>X602</text>
<text>XTAL101</text>
<wire x1="176" y1="122" x2="176" y2="36" width="0.1" layer="20"/>
<wire x1="174" y1="124" x2="10" y2="124" width="0.1" layer="20"/>
<wire x1="8" y1="122" x2="8" y2="36" width="0.1" layer="20"/>
<wire x1="10" y1="34" x2="174" y2="34" width="0.1" layer="20"/>
<wire x1="0" y1="132" x2="184" y2="132" width="0.1" layer="20"/>
<wire x1="184" y1="132" x2="184" y2="0" width="0.1" layer="20"/>
<wire x1="184" y1="0" x2="0" y2="0" width="0.1" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="132" width="0.1" layer="20"/>
<wire x1="23" y1="32" x2="9" y2="32" width="0.1" layer="20"/>
<wire x1="8" y1="31" x2="8" y2="12.5" width="0.1" layer="20"/>
<wire x1="24" y1="12.5" x2="24" y2="31" width="0.1" layer="20"/>
<wire x1="23" y1="11.5" x2="9" y2="11.5" width="0.1" layer="20"/>
<text>TOP</text>
<text>BOT</text>
<text>REF</text>
<text>REF</text>
<text>Heatsink</text>
<text>glue area</text>
<text>A4988</text>
<text>V1.1DE</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>IC1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<wire x1="41" y1="32" x2="27" y2="32" width="0.1" layer="20"/>
<wire x1="26" y1="31" x2="26" y2="12.5" width="0.1" layer="20"/>
<wire x1="42" y1="12.5" x2="42" y2="31" width="0.1" layer="20"/>
<wire x1="41" y1="11.5" x2="27" y2="11.5" width="0.1" layer="20"/>
<text>TOP</text>
<text>BOT</text>
<text>REF</text>
<text>REF</text>
<text>Heatsink</text>
<text>glue area</text>
<text>A4988</text>
<text>V1.1DE</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>IC1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<wire x1="59" y1="32" x2="45" y2="32" width="0.1" layer="20"/>
<wire x1="44" y1="31" x2="44" y2="12.5" width="0.1" layer="20"/>
<wire x1="60" y1="12.5" x2="60" y2="31" width="0.1" layer="20"/>
<wire x1="59" y1="11.5" x2="45" y2="11.5" width="0.1" layer="20"/>
<text>TOP</text>
<text>BOT</text>
<text>REF</text>
<text>REF</text>
<text>Heatsink</text>
<text>glue area</text>
<text>A4988</text>
<text>V1.1DE</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>IC1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<wire x1="77" y1="32" x2="63" y2="32" width="0.1" layer="20"/>
<wire x1="62" y1="31" x2="62" y2="12.5" width="0.1" layer="20"/>
<wire x1="78" y1="12.5" x2="78" y2="31" width="0.1" layer="20"/>
<wire x1="77" y1="11.5" x2="63" y2="11.5" width="0.1" layer="20"/>
<text>TOP</text>
<text>BOT</text>
<text>REF</text>
<text>REF</text>
<text>Heatsink</text>
<text>glue area</text>
<text>A4988</text>
<text>V1.1DE</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>IC1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<wire x1="95" y1="32" x2="81" y2="32" width="0.1" layer="20"/>
<wire x1="80" y1="31" x2="80" y2="12.5" width="0.1" layer="20"/>
<wire x1="96" y1="12.5" x2="96" y2="31" width="0.1" layer="20"/>
<wire x1="95" y1="11.5" x2="81" y2="11.5" width="0.1" layer="20"/>
<text>TOP</text>
<text>BOT</text>
<text>REF</text>
<text>REF</text>
<text>Heatsink</text>
<text>glue area</text>
<text>A4988</text>
<text>V1.1DE</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>IC1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<wire x1="113" y1="32" x2="99" y2="32" width="0.1" layer="20"/>
<wire x1="98" y1="31" x2="98" y2="12.5" width="0.1" layer="20"/>
<wire x1="114" y1="12.5" x2="114" y2="31" width="0.1" layer="20"/>
<wire x1="113" y1="11.5" x2="99" y2="11.5" width="0.1" layer="20"/>
<text>TOP</text>
<text>BOT</text>
<text>REF</text>
<text>REF</text>
<text>Heatsink</text>
<text>glue area</text>
<text>A4988</text>
<text>V1.1DE</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>IC1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<wire x1="122" y1="21" x2="145" y2="21" width="0.1" layer="20"/>
<wire x1="147" y1="23" x2="147" y2="30" width="0.1" layer="20"/>
<wire x1="120" y1="30" x2="120" y2="23" width="0.1" layer="20"/>
<text>BOT</text>
<text>TOP</text>
<text>+5V</text>
<text>OUT</text>
<text>GND</text>
<text>C</text>
<text>Opto-Endstop</text>
<text>V1.0 20120320_DE</text>
<text>C1</text>
<text>IC1</text>
<text>LED1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>T1</text>
<hole x="124.5" y="26.3" drill="3.2"/>
<hole x="142.5" y="26.3" drill="3.2"/>
<wire x1="122" y1="32" x2="145" y2="32" width="0.1" layer="20"/>
<wire x1="151" y1="21" x2="174" y2="21" width="0.1" layer="20"/>
<wire x1="176" y1="23" x2="176" y2="30" width="0.1" layer="20"/>
<wire x1="149" y1="30" x2="149" y2="23" width="0.1" layer="20"/>
<text>BOT</text>
<text>TOP</text>
<text>+5V</text>
<text>OUT</text>
<text>GND</text>
<text>C</text>
<text>Opto-Endstop</text>
<text>V1.0 20120320_DE</text>
<text>C1</text>
<text>IC1</text>
<text>LED1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>T1</text>
<hole x="153.5" y="26.3" drill="3.2"/>
<hole x="171.5" y="26.3" drill="3.2"/>
<wire x1="151" y1="32" x2="174" y2="32" width="0.1" layer="20"/>
<wire x1="151" y1="8" x2="174" y2="8" width="0.1" layer="20"/>
<wire x1="176" y1="10" x2="176" y2="17" width="0.1" layer="20"/>
<wire x1="149" y1="17" x2="149" y2="10" width="0.1" layer="20"/>
<text>BOT</text>
<text>TOP</text>
<text>+5V</text>
<text>OUT</text>
<text>GND</text>
<text>C</text>
<text>Opto-Endstop</text>
<text>V1.0 20120320_DE</text>
<text>C1</text>
<text>IC1</text>
<text>LED1</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>T1</text>
<hole x="153.5" y="13.3" drill="3.2"/>
<hole x="171.5" y="13.3" drill="3.2"/>
<wire x1="151" y1="19" x2="174" y2="19" width="0.1" layer="20"/>
<text>(130 | 10)</text>
<text>(3,5 | 128,5)</text>
<text>(181 | 120)</text>
<text>6x Stepper_Driver</text>
<text>3x Endstop</text>
<text>1x Controller</text>
<text>Sanguino_STB_V51_panel</text>
<text>03.04.2013</text>
<wire x1="8" y1="122" x2="10" y2="124" width="0.1" layer="20" curve="-90"/>
<wire x1="174" y1="124" x2="176" y2="122" width="0.1" layer="20" curve="-90"/>
<wire x1="176" y1="36" x2="174" y2="34" width="0.1" layer="20" curve="-90"/>
<wire x1="10" y1="34" x2="8" y2="36" width="0.1" layer="20" curve="-90"/>
<wire x1="120" y1="30" x2="122" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="145" y1="32" x2="147" y2="30" width="0.1" layer="20" curve="-90"/>
<wire x1="147" y1="23" x2="145" y2="21" width="0.1" layer="20" curve="-90"/>
<wire x1="151" y1="21" x2="149" y2="23" width="0.1" layer="20" curve="-90"/>
<wire x1="122" y1="21" x2="120" y2="23" width="0.1" layer="20" curve="-90"/>
<wire x1="176" y1="23" x2="174" y2="21" width="0.1" layer="20" curve="-90"/>
<wire x1="174" y1="32" x2="176" y2="30" width="0.1" layer="20" curve="-90"/>
<wire x1="149" y1="30" x2="151" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="149" y1="17" x2="151" y2="19" width="0.1" layer="20" curve="-90"/>
<wire x1="174" y1="19" x2="176" y2="17" width="0.1" layer="20" curve="-90"/>
<wire x1="176" y1="10" x2="174" y2="8" width="0.1" layer="20" curve="-90"/>
<wire x1="151" y1="8" x2="149" y2="10" width="0.1" layer="20" curve="-90"/>
<wire x1="8" y1="31" x2="9" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="8" y1="31" x2="9" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="26" y1="31" x2="27" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="23" y1="32" x2="24" y2="31" width="0.1" layer="20" curve="-90"/>
<wire x1="41" y1="32" x2="42" y2="31" width="0.1" layer="20" curve="-90"/>
<wire x1="44" y1="31" x2="45" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="59" y1="32" x2="60" y2="31" width="0.1" layer="20" curve="-90"/>
<wire x1="62" y1="31" x2="63" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="77" y1="32" x2="78" y2="31" width="0.1" layer="20" curve="-90"/>
<wire x1="80" y1="31" x2="81" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="98" y1="31" x2="99" y2="32" width="0.1" layer="20" curve="-90"/>
<wire x1="95" y1="32" x2="96" y2="31" width="0.1" layer="20" curve="-90"/>
<wire x1="113" y1="32" x2="114" y2="31" width="0.1" layer="20" curve="-90"/>
<wire x1="114" y1="12.5" x2="113" y2="11.5" width="0.1" layer="20" curve="-90"/>
<wire x1="99" y1="11.5" x2="98" y2="12.5" width="0.1" layer="20" curve="-90"/>
<wire x1="96" y1="12.5" x2="95" y2="11.5" width="0.1" layer="20" curve="-90"/>
<wire x1="81" y1="11.5" x2="80" y2="12.5" width="0.1" layer="20" curve="-90"/>
<wire x1="78" y1="12.5" x2="77" y2="11.5" width="0.1" layer="20" curve="-90"/>
<wire x1="63" y1="11.5" x2="62" y2="12.5" width="0.1" layer="20" curve="-90"/>
<wire x1="60" y1="12.5" x2="59" y2="11.5" width="0.1" layer="20" curve="-90"/>
<wire x1="45" y1="11.5" x2="44" y2="12.5" width="0.1" layer="20" curve="-90"/>
<wire x1="42" y1="12.5" x2="41" y2="11.5" width="0.1" layer="20" curve="-90"/>
<wire x1="27" y1="11.5" x2="26" y2="12.5" width="0.1" layer="20" curve="-90"/>
<wire x1="24" y1="12.5" x2="23" y2="11.5" width="0.1" layer="20" curve="-90"/>
<wire x1="9" y1="11.5" x2="8" y2="12.5" width="0.1" layer="20" curve="-90"/>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>184</text>
<text>132</text>
<text>F601</text>
<text>Fuse</text>
<text>+12..24V</text>
<text>GND</text>
<text>GND</text>
<text>-</text>
<text>Ser.No.:</text>
<text>Test:</text>
<text>RepRap</text>
<text>www.reprap-electronics.de</text>
<text>Bootloader:</text>
<text>http://www.reprap-electronics.de</text>
<text>F501</text>
<text>Hotend Fuse</text>
<text>Main-</text>
<text>Recommended Fuse Values</text>
<text>12V Supply:</text>
<text>24V Supply:</text>
<text>Main 25A, Hotend 7.5A</text>
<text>Main 15A, Hotend 5A</text>
</plain>
<libraries>
<library name="avr-7">
<packages>
<package name="TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="AVR-JTAG-10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 10 Pin, 0.1" Straight</description>
</package>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pololu-allegro">
<packages>
<package name="POLOLU-ALLEGRO-PTH">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="MOLEX-1X4">
</package>
<package name="MOLEX-1X3">
</package>
<package name="MOLEX-1X2">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="display_ea_dogm128">
<packages>
<package name="E_DOG-M_DISPLAY">
<description>Electronic Assembly LCD Display&lt;p&gt;

128x64 Pixel&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="ST_Automotive">
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="Project7264">
<packages>
<package name="TPD2E001-DRL">
<description>TPD2E001 ESD-protection diode array,DRL-Package, RM  0,5mm, H=0,6mm</description>
</package>
</packages>
</library>
<library name="ftdichip">
<packages>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt; SSOP-28&lt;p&gt;
http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SMA">
<description>&lt;b&gt;SMA&lt;/b&gt; CASE 403D-02&lt;p&gt;
Source: http://www.onsemi.com/pub_link/Collateral/MBRA340T3-D.PDF</description>
</package>
</packages>
</library>
<library name="transistor-power">
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="atx-power-supply">
<packages>
<package name="MINIFITJR-4-VERTICAL">
<description>&lt;b&gt;Mini FIT connector 4 pol&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transil">
<packages>
<package name="SMAJ">
<description>ST Transil Diode&lt;br&gt;
SMAJ Package</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<packages>
<package name="W237-4">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="switch-alps">
<description>ALPS Switch from Markus Faust &amp;lt;mfaust@htwm.de&amp;gt;&lt;p&gt;
Source: EC12E.scr from eagle.support.ger on news.cadsoft.de at 08.10.2007</description>
<packages>
<package name="ALPS_EC12E_SW">
<description>ALPS rotary encoder&lt;br&gt;
EC12E series with push-on switch</description>
</package>
</packages>
</library>
<library name="st-microelectronics">
<description>&lt;b&gt;ST Microelectronics Devices&lt;/b&gt;&lt;p&gt;
Microcontrollers,  I2C components, linear devices&lt;p&gt;
http://www.st.com&lt;p&gt;
&lt;i&gt;Include st-microelectronics-2.lbr, st-microelectronics-3.lbr.&lt;p&gt;&lt;/i&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HSOP8">
<description>&lt;b&gt;HSOP 08&lt;/b&gt; (Exposed pad)&lt;p&gt;
Source: http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00002851.pdf</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
Source: INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
</packages>
</library>
<library name="inductor-coilcraft">
<description>&lt;b&gt;Coilcraft SMD Inductors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO3316P">
<description>&lt;b&gt;COILCRAFT&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="reprap">
<packages>
<package name="MICRO_SD_MOLEX_473093351">
<description>MOLEX µSD Connector&lt;br&gt;
SD-47309-001</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="MOLEX_52892-3095">
<description>Molex Folien Steckverbinder&lt;br&gt;
52892-3095</description>
</package>
<package name="JST-BSB-PH">
<description>JST&lt;br&gt;
JST-BSB-PH Connector 2mm</description>
</package>
<package name="MCCQ-122">
<description>Fuse Holder&lt;br&gt;
MCCQ-122</description>
</package>
</packages>
</library>
<library name="vito_lib">
<packages>
<package name="SD-47346-001">
<description>MOLEX Micro USB Connector&lt;br&gt;
Part No.: SD-47346-001</description>
</package>
</packages>
</library>
<library name="droptime">
<packages>
<package name="MJTP1236">
<description>Taster Package&lt;p&gt;
MJTP1236 / PHAP3305</description>
</package>
</packages>
</library>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="infineon_reprap">
<packages>
<package name="TDSON-8">
<description>Infineon&lt;br&gt;
PG-TDSON-8 Package</description>
</package>
</packages>
</library>
<library name="special">
<packages>
<package name="L6055">
</package>
</packages>
</library>
<library name="rl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="LBRstepstick">
<packages>
<package name="POLOLU-ALLEGRO_CLONOLU">
</package>
<package name="ALLEGRO_QFN28ET">
<description>&lt;b&gt;28 Pin QFN ET&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 32&lt;/i&gt;&lt;br&gt;
Source: http://www.allegromicro.com/en/Products/Part_Numbers/4983/4983.pdf</description>
</package>
<package name="PVZ2A">
</package>
</packages>
</library>
<library name="opto">
<packages>
<package name="EE-SX1109">
<description>EE-SX1109 Photomicrosensor&lt;br&gt;
Gabellichtschranke SMD&lt;br&gt;
Schlitzbreite: 3mm, Schlitztiefe 3.5mm&lt;br&gt;
Optische Öffnung: 0.5mm x 1.0mm&lt;br&gt;
Omron</description>
</package>
</packages>
</library>
<library name="graphics_logos">
<packages>
<package name="EASY_EL_LOGO_50MM">
</package>
<package name="QR_20MM">
<description>http://www.reprap-electronics.de</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC101" library="avr-7" package="TQFP44" value="MEGA164P/324P/644P-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="rcl" package="C0805K" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R101" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C104" library="rcl" package="C0805K" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C107" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C109" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C106" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C103" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C108" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C101" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R102" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C110" library="rcl" package="C0805K" value="nc">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP102" library="avr-7" package="AVR-JTAG-10" value="AVR-JTAG-10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTAL101" library="crystal" package="HC49U-V" value="20.00MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X202" library="pololu-allegro" package="POLOLU-ALLEGRO-PTH" value="POLOLU-X">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X203" library="pololu-allegro" package="POLOLU-ALLEGRO-PTH" value="POLOLU-Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X201" library="pololu-allegro" package="POLOLU-ALLEGRO-PTH" value="POLOLU-Z">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP205" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="JP206" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="JP207" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="X204" library="pololu-allegro" package="POLOLU-ALLEGRO-PTH" value="POLOLU-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP210" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="JP204" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="C207" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C208" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C211" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C217" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R201" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R202" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R203" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R204" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C210" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C209" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C212" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C219" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C205" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C206" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C202" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C215" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C203" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C204" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C201" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C213" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP301" library="SparkFun" package="MOLEX-1X3" value=""/>
<element name="JP302" library="SparkFun" package="MOLEX-1X3" value=""/>
<element name="JP303" library="SparkFun" package="MOLEX-1X3" value=""/>
<element name="R301" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R303" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R302" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C301" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C302" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C303" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP101" library="avr-7" package="AVR-ISP-6" value="AVR-ISP-6VERT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R304" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R306" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C306" library="rcl" package="C0805K" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C304" library="rcl" package="C0805K" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP304" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="JP306" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="LCD401" library="display_ea_dogm128" package="E_DOG-M_DISPLAY" value="DOG-M128">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C413" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C420" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C424" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C421" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C422" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C423" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C416" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C414" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C425" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C426" library="rcl" package="C0805K" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C412" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R408" library="rcl" package="R0805" value="82">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R409" library="rcl" package="R0805" value="82">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R410" library="rcl" package="R0805" value="82">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C401" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R407" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C411" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C417" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC403" library="ST_Automotive" package="SOT223" value="LD1117S33CTR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C402" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C407" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C405" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R401" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R402" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED402" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED403" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R405" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R406" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C404" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C406" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C408" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C409" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC402" library="Project7264" package="TPD2E001-DRL" value="TPD2E001DRLR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R404" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R403" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC404" library="ftdichip" package="SSOP28" value="FT232RL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP502" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="JP503" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="JP504" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="R511" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R504" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R510" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R503" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R512" library="rcl" package="R1206" value="nc">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C503" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R507" library="rcl" package="R1206" value="nc">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C502" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R506" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R505" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP501" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="T501" library="transistor-power" package="SO-08" value="DMS3016SSS-13">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C602" library="SparkFun" package="CPOL-RADIAL-1000UF-25V" value="1000uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X602" library="atx-power-supply" package="MINIFITJR-4-VERTICAL" value="ATX-4VERTICAL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C603" library="rcl" package="C1206K" value="10µF (GRM31CR6YA106KA12L)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C601" library="rcl" package="C1206K" value="10µF (GRM31CR6YA106KA12L)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED602" library="led" package="CHIPLED_0805" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R606" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C604" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D601" library="transil" package="SMAJ" value="SMAJ13CA-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D602" library="transil" package="SMAJ" value="SMAJ6.5CA-TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X601" library="con-wago-500" package="W237-4" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="H602" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H601" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="SW401" library="switch-alps" package="ALPS_EC12E_SW" value="EC12E_SW">
<attribute name="OC_NEWARK" value="74M1068"/>
<attribute name="MPN" value="EC12E2424407"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1520813"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C105" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T503" library="transistor-power" package="SO-08" value="DMS3016SSS-13">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R305" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C305" library="rcl" package="C0805K" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP305" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="R515" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R514" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R516" library="rcl" package="R1206" value="nc">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C504" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T504" library="transistor-power" package="SO-08" value="DMS3016SSS-13">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X205" library="pololu-allegro" package="POLOLU-ALLEGRO-PTH" value="POLOLU-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP211" library="SparkFun" package="MOLEX-1X4" value=""/>
<element name="C218" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R205" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C220" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C216" library="rcl" package="PANASONIC_A" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C214" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC601" library="st-microelectronics" package="HSOP8" value="L5973D">
<attribute name="MPN" value="L5973D"/>
<attribute name="MF" value="STMICROELECTRONICS"/>
<attribute name="OC_FARNELL" value="1077145"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C613" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C612" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C611" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C610" library="rcl" package="C0805K" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C609" library="rcl" package="PANASONIC_D" value="220µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L601" library="inductor-coilcraft" package="DO3316P" value="P0751.473NLT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R603" library="rcl" package="R0805" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R604" library="rcl" package="R0805" value="2k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C607" library="rcl" package="PANASONIC_G" value="220µF/ESR max. 500mOhm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D604" library="diode" package="SMB" value="STPS2L40U">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C606" library="rcl" package="C0805K" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C605" library="rcl" package="C0805K" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R601" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED401" library="led" package="CHIPLED_0805" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R411" library="rcl" package="R0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED502" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R508" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED501" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R502" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED503" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R509" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED504" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R513" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED101" library="led" package="CHIPLED_0805" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R104" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R103" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T101" library="transistor" package="SOT23-BEC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP505" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="JP506" library="SparkFun" package="MOLEX-1X2" value=""/>
<element name="JP202" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP203" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP201" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP208" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP209" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R501" library="rcl" package="R1206" value="nc">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C501" library="rcl" package="C0805K" value="4,7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X402" library="reprap" package="MICRO_SD_MOLEX_473093351" value="MICRO_SD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R517" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X401" library="vito_lib" package="SD-47346-001" value="MICRO-USB-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP507" library="SparkFun" package="MOLEX-1X3" value=""/>
<element name="SW101" library="droptime" package="MJTP1236" value="MJTP1236 - lang">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R518" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C608" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T505" library="reprap" package="SOT23" value="NX2301P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC401" library="40xx" package="SO16" value="4050D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="T502" library="infineon_reprap" package="TDSON-8" value="BSC025N03LS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L602" library="special" package="L6055" value="100µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D502" library="diode" package="SMA" value="MBRA340T3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D503" library="diode" package="SMA" value="MBRA340T3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D504" library="diode" package="SMA" value="MBRA340T3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D501" library="diode" package="SMA" value="MBRA340T3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC602" library="v-reg" package="D2PACK" value="LD117AD2MTR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X403" library="reprap" package="MOLEX_52892-3095" value="MOLEX_FLEX_52892-3095">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X404" library="reprap" package="JST-BSB-PH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R412" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X" library="LBRstepstick" package="POLOLU-ALLEGRO_CLONOLU" value="POLOLU-ALLEGRO_CLONOLU">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="LBRstepstick" package="ALLEGRO_QFN28ET" value="ALLEGRO_A4983">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="LBRstepstick" package="PVZ2A" value="PVZ2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="LBRstepstick" package="POLOLU-ALLEGRO_CLONOLU" value="POLOLU-ALLEGRO_CLONOLU">
<attribute name="VALUE"/>
</element>
<element name="C14" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="LBRstepstick" package="ALLEGRO_QFN28ET" value="ALLEGRO_A4983">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="LBRstepstick" package="PVZ2A" value="PVZ2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="LBRstepstick" package="POLOLU-ALLEGRO_CLONOLU" value="POLOLU-ALLEGRO_CLONOLU">
<attribute name="VALUE"/>
</element>
<element name="C21" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="LBRstepstick" package="ALLEGRO_QFN28ET" value="ALLEGRO_A4983">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="LBRstepstick" package="PVZ2A" value="PVZ2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="SparkFun" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="LBRstepstick" package="POLOLU-ALLEGRO_CLONOLU" value="POLOLU-ALLEGRO_CLONOLU">
<attribute name="VALUE"/>
</element>
<element name="C28" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="LBRstepstick" package="ALLEGRO_QFN28ET" value="ALLEGRO_A4983">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="LBRstepstick" package="PVZ2A" value="PVZ2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="SparkFun" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="LBRstepstick" package="POLOLU-ALLEGRO_CLONOLU" value="POLOLU-ALLEGRO_CLONOLU">
<attribute name="VALUE"/>
</element>
<element name="C35" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="LBRstepstick" package="ALLEGRO_QFN28ET" value="ALLEGRO_A4983">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="LBRstepstick" package="PVZ2A" value="PVZ2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="SparkFun" package="1206" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rl" package="R0603" value="220n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="rcl" package="R0805" value="0,075 330mW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="LBRstepstick" package="POLOLU-ALLEGRO_CLONOLU" value="POLOLU-ALLEGRO_CLONOLU">
<attribute name="VALUE"/>
</element>
<element name="C42" library="rl" package="R0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="LBRstepstick" package="ALLEGRO_QFN28ET" value="ALLEGRO_A4983">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="LBRstepstick" package="PVZ2A" value="PVZ2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="rcl" package="R0805" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC817">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="rcl" package="R0805" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X6" library="opto" package="EE-SX1109" value="EE-SX1109">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_1206" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rcl" package="R0805" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor" package="SOT23" value="BC817">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="rcl" package="R0805" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="opto" package="EE-SX1109" value="EE-SX1109">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_1206" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="rcl" package="R0805" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0805K" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="transistor" package="SOT23" value="BC817">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="rcl" package="R0805" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X8" library="opto" package="EE-SX1109" value="EE-SX1109">
<attribute name="VALUE"/>
</element>
<element name="F601" library="reprap" package="MCCQ-122" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$61" library="graphics_logos" package="EASY_EL_LOGO_50MM" value=""/>
<element name="F501" library="reprap" package="MCCQ-122" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$62" library="graphics_logos" package="QR_20MM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC101" pad="6"/>
<contactref element="IC101" pad="18"/>
<contactref element="IC101" pad="28"/>
<contactref element="IC101" pad="39"/>
<contactref element="C102" pad="1"/>
<contactref element="C104" pad="2"/>
<contactref element="C107" pad="1"/>
<contactref element="C109" pad="1"/>
<contactref element="C103" pad="1"/>
<contactref element="C106" pad="1"/>
<contactref element="C108" pad="1"/>
<contactref element="C101" pad="-"/>
<contactref element="C110" pad="2"/>
<contactref element="JP102" pad="2"/>
<contactref element="JP102" pad="10"/>
<contactref element="JP101" pad="6"/>
<contactref element="C105" pad="-"/>
<contactref element="X203" pad="GNDVDD"/>
<contactref element="X203" pad="GNDMOT"/>
<contactref element="X202" pad="GNDVDD"/>
<contactref element="X202" pad="GNDMOT"/>
<contactref element="X201" pad="GNDVDD"/>
<contactref element="X201" pad="GNDMOT"/>
<contactref element="C211" pad="-"/>
<contactref element="C208" pad="-"/>
<contactref element="C207" pad="-"/>
<contactref element="X204" pad="GNDVDD"/>
<contactref element="X204" pad="GNDMOT"/>
<contactref element="C217" pad="-"/>
<contactref element="R203" pad="2"/>
<contactref element="R204" pad="2"/>
<contactref element="R201" pad="2"/>
<contactref element="C209" pad="1"/>
<contactref element="C210" pad="1"/>
<contactref element="C212" pad="1"/>
<contactref element="C219" pad="1"/>
<contactref element="C205" pad="-"/>
<contactref element="C206" pad="-"/>
<contactref element="C202" pad="-"/>
<contactref element="C215" pad="-"/>
<contactref element="C203" pad="2"/>
<contactref element="C204" pad="2"/>
<contactref element="C201" pad="2"/>
<contactref element="C213" pad="2"/>
<contactref element="X205" pad="GNDVDD"/>
<contactref element="X205" pad="GNDMOT"/>
<contactref element="C218" pad="-"/>
<contactref element="R205" pad="2"/>
<contactref element="C220" pad="1"/>
<contactref element="C216" pad="-"/>
<contactref element="C214" pad="2"/>
<contactref element="JP303" pad="3"/>
<contactref element="JP302" pad="3"/>
<contactref element="JP301" pad="3"/>
<contactref element="C301" pad="1"/>
<contactref element="C302" pad="1"/>
<contactref element="C303" pad="1"/>
<contactref element="C304" pad="1"/>
<contactref element="JP304" pad="2"/>
<contactref element="C306" pad="1"/>
<contactref element="JP306" pad="2"/>
<contactref element="C305" pad="1"/>
<contactref element="JP305" pad="2"/>
<contactref element="C413" pad="2"/>
<contactref element="C412" pad="-"/>
<contactref element="LCD401" pad="33"/>
<contactref element="LCD401" pad="26"/>
<contactref element="C421" pad="2"/>
<contactref element="C426" pad="2"/>
<contactref element="C425" pad="2"/>
<contactref element="C424" pad="2"/>
<contactref element="C423" pad="2"/>
<contactref element="C422" pad="2"/>
<contactref element="C401" pad="1"/>
<contactref element="C411" pad="1"/>
<contactref element="C417" pad="1"/>
<contactref element="IC403" pad="1"/>
<contactref element="C402" pad="1"/>
<contactref element="C407" pad="-"/>
<contactref element="C405" pad="1"/>
<contactref element="C406" pad="1"/>
<contactref element="C408" pad="1"/>
<contactref element="C409" pad="-"/>
<contactref element="R403" pad="2"/>
<contactref element="IC402" pad="4"/>
<contactref element="R402" pad="2"/>
<contactref element="C404" pad="1"/>
<contactref element="IC404" pad="25"/>
<contactref element="IC404" pad="7"/>
<contactref element="IC404" pad="18"/>
<contactref element="IC404" pad="21"/>
<contactref element="IC404" pad="26"/>
<contactref element="SW401" pad="E"/>
<contactref element="SW401" pad="GND2"/>
<contactref element="SW401" pad="GND1"/>
<contactref element="SW401" pad="C"/>
<contactref element="R408" pad="2"/>
<contactref element="R409" pad="2"/>
<contactref element="R410" pad="2"/>
<contactref element="R504" pad="2"/>
<contactref element="JP504" pad="2"/>
<contactref element="R507" pad="2"/>
<contactref element="C502" pad="1"/>
<contactref element="T501" pad="1"/>
<contactref element="T501" pad="3"/>
<contactref element="T501" pad="2"/>
<contactref element="R505" pad="1"/>
<contactref element="JP503" pad="2"/>
<contactref element="X602" pad="1"/>
<contactref element="X602" pad="2"/>
<contactref element="X601" pad="4"/>
<contactref element="X601" pad="3"/>
<contactref element="LED602" pad="C"/>
<contactref element="C602" pad="2"/>
<contactref element="C604" pad="1"/>
<contactref element="C603" pad="1"/>
<contactref element="C601" pad="1"/>
<contactref element="D601" pad="P$2"/>
<contactref element="D602" pad="P$2"/>
<contactref element="C612" pad="1"/>
<contactref element="C613" pad="-"/>
<contactref element="C611" pad="1"/>
<contactref element="C610" pad="1"/>
<contactref element="C609" pad="-"/>
<contactref element="R604" pad="2"/>
<contactref element="IC601" pad="3"/>
<contactref element="IC601" pad="7"/>
<contactref element="C607" pad="-"/>
<contactref element="D604" pad="A"/>
<contactref element="R601" pad="2"/>
<contactref element="C605" pad="1"/>
<contactref element="IC601" pad="EXP"/>
<contactref element="LED401" pad="C"/>
<contactref element="LED502" pad="C"/>
<contactref element="LED501" pad="C"/>
<contactref element="LED101" pad="C"/>
<contactref element="R202" pad="2"/>
<contactref element="R501" pad="2"/>
<contactref element="C501" pad="1"/>
<contactref element="X402" pad="G1"/>
<contactref element="X402" pad="G2"/>
<contactref element="X402" pad="G1"/>
<contactref element="X402" pad="G2"/>
<contactref element="X402" pad="6"/>
<contactref element="X401" pad="5"/>
<contactref element="JP507" pad="2"/>
<contactref element="SW101" pad="2"/>
<contactref element="SW101" pad="GND1"/>
<contactref element="SW101" pad="GND2"/>
<contactref element="C608" pad="1"/>
<contactref element="IC401" pad="8"/>
<contactref element="T502" pad="1"/>
<contactref element="T502" pad="2"/>
<contactref element="T502" pad="3"/>
<contactref element="IC602" pad="1"/>
<contactref element="X403" pad="14"/>
<contactref element="X403" pad="21"/>
<contactref element="X403" pad="30"/>
<contactref element="R412" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="X" pad="GND$1"/>
<contactref element="X" pad="GND$2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="EXP"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="25"/>
<contactref element="R4" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="X1" pad="GND$1"/>
<contactref element="X1" pad="GND$2"/>
<contactref element="C14" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="EXP"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="25"/>
<contactref element="R14" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="X2" pad="GND$1"/>
<contactref element="X2" pad="GND$2"/>
<contactref element="C21" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="EXP"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="20"/>
<contactref element="IC3" pad="25"/>
<contactref element="R21" pad="2"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C24" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="X3" pad="GND$1"/>
<contactref element="X3" pad="GND$2"/>
<contactref element="C28" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC4" pad="18"/>
<contactref element="IC4" pad="EXP"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC4" pad="25"/>
<contactref element="R28" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="X4" pad="GND$1"/>
<contactref element="X4" pad="GND$2"/>
<contactref element="C35" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC5" pad="18"/>
<contactref element="IC5" pad="EXP"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC5" pad="25"/>
<contactref element="R35" pad="2"/>
<contactref element="C36" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C38" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="X5" pad="GND$1"/>
<contactref element="X5" pad="GND$2"/>
<contactref element="C42" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="18"/>
<contactref element="IC6" pad="EXP"/>
<contactref element="IC6" pad="7"/>
<contactref element="IC6" pad="20"/>
<contactref element="IC6" pad="25"/>
<contactref element="R42" pad="2"/>
<contactref element="C43" pad="1"/>
<contactref element="X6" pad="CA"/>
<contactref element="X6" pad="E"/>
<contactref element="LED1" pad="C"/>
<contactref element="C44" pad="1"/>
<contactref element="X7" pad="CA"/>
<contactref element="X7" pad="E"/>
<contactref element="LED2" pad="C"/>
<contactref element="C45" pad="1"/>
<contactref element="X8" pad="CA"/>
<contactref element="X8" pad="E"/>
<contactref element="LED3" pad="C"/>
<contactref element="F501" pad="1"/>
<contactref element="F501" pad="3"/>
</signal>
<signal name="!RESET">
<contactref element="JP102" pad="6"/>
<contactref element="IC101" pad="4"/>
<contactref element="R102" pad="2"/>
<contactref element="C110" pad="1"/>
<contactref element="JP101" pad="5"/>
<contactref element="SW101" pad="1"/>
</signal>
<signal name="5V">
<contactref element="IC101" pad="38"/>
<contactref element="IC101" pad="17"/>
<contactref element="IC101" pad="5"/>
<contactref element="IC101" pad="27"/>
<contactref element="C109" pad="2"/>
<contactref element="C103" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="C108" pad="2"/>
<contactref element="C101" pad="+"/>
<contactref element="R102" pad="1"/>
<contactref element="R101" pad="2"/>
<contactref element="JP102" pad="4"/>
<contactref element="JP101" pad="2"/>
<contactref element="X202" pad="VDD"/>
<contactref element="C205" pad="+"/>
<contactref element="C203" pad="1"/>
<contactref element="X203" pad="VDD"/>
<contactref element="C206" pad="+"/>
<contactref element="C204" pad="1"/>
<contactref element="X201" pad="VDD"/>
<contactref element="C202" pad="+"/>
<contactref element="C201" pad="1"/>
<contactref element="X204" pad="VDD"/>
<contactref element="C215" pad="+"/>
<contactref element="C213" pad="1"/>
<contactref element="X205" pad="VDD"/>
<contactref element="C216" pad="+"/>
<contactref element="C214" pad="1"/>
<contactref element="JP303" pad="2"/>
<contactref element="JP302" pad="2"/>
<contactref element="JP301" pad="2"/>
<contactref element="R304" pad="1"/>
<contactref element="R306" pad="1"/>
<contactref element="R305" pad="1"/>
<contactref element="IC403" pad="3"/>
<contactref element="C402" pad="2"/>
<contactref element="LCD401" pad="1"/>
<contactref element="LCD401" pad="2"/>
<contactref element="LCD401" pad="3"/>
<contactref element="R405" pad="1"/>
<contactref element="R406" pad="1"/>
<contactref element="C409" pad="+"/>
<contactref element="C408" pad="2"/>
<contactref element="C406" pad="2"/>
<contactref element="IC404" pad="20"/>
<contactref element="IC404" pad="4"/>
<contactref element="JP504" pad="1"/>
<contactref element="R606" pad="1"/>
<contactref element="D602" pad="P$1"/>
<contactref element="C612" pad="2"/>
<contactref element="C613" pad="+"/>
<contactref element="T101" pad="E"/>
<contactref element="JP202" pad="2"/>
<contactref element="JP202" pad="4"/>
<contactref element="JP202" pad="6"/>
<contactref element="JP203" pad="6"/>
<contactref element="JP203" pad="4"/>
<contactref element="JP203" pad="2"/>
<contactref element="JP201" pad="4"/>
<contactref element="JP201" pad="6"/>
<contactref element="JP201" pad="2"/>
<contactref element="JP208" pad="6"/>
<contactref element="JP208" pad="4"/>
<contactref element="JP208" pad="2"/>
<contactref element="JP209" pad="4"/>
<contactref element="JP209" pad="2"/>
<contactref element="JP209" pad="6"/>
<contactref element="R518" pad="1"/>
<contactref element="T505" pad="2"/>
<contactref element="IC602" pad="2"/>
<contactref element="X404" pad="1"/>
</signal>
<signal name="PB7-SCK">
<contactref element="IC101" pad="3"/>
<contactref element="JP101" pad="3"/>
<contactref element="IC401" pad="9"/>
</signal>
<signal name="PB6-MISO">
<contactref element="IC101" pad="2"/>
<contactref element="JP101" pad="1"/>
<contactref element="R401" pad="1"/>
</signal>
<signal name="PB5-MOSI">
<contactref element="IC101" pad="1"/>
<contactref element="JP101" pad="4"/>
<contactref element="IC401" pad="3"/>
</signal>
<signal name="E-THERM0">
<contactref element="IC101" pad="30"/>
<contactref element="R304" pad="2"/>
<contactref element="C304" pad="2"/>
<contactref element="JP304" pad="1"/>
</signal>
<signal name="B-THERM">
<contactref element="IC101" pad="31"/>
<contactref element="R306" pad="2"/>
<contactref element="C306" pad="2"/>
<contactref element="JP306" pad="1"/>
</signal>
<signal name="A0">
<contactref element="IC101" pad="37"/>
<contactref element="IC401" pad="14"/>
</signal>
<signal name="A1">
<contactref element="IC101" pad="36"/>
<contactref element="IC401" pad="11"/>
</signal>
<signal name="A2">
<contactref element="IC101" pad="35"/>
<contactref element="IC401" pad="5"/>
</signal>
<signal name="E1-DIR">
<contactref element="IC101" pad="34"/>
<contactref element="X205" pad="DIR"/>
</signal>
<signal name="E1-STEP">
<contactref element="IC101" pad="33"/>
<contactref element="X205" pad="STEP"/>
</signal>
<signal name="PB4-PWM">
<contactref element="IC101" pad="44"/>
<contactref element="R506" pad="2"/>
<contactref element="R508" pad="2"/>
</signal>
<signal name="!ENC_1">
<contactref element="IC101" pad="12"/>
<contactref element="SW401" pad="A"/>
</signal>
<signal name="!ENC_2">
<contactref element="IC101" pad="11"/>
<contactref element="SW401" pad="B"/>
</signal>
<signal name="AIFO">
<contactref element="IC101" pad="9"/>
<contactref element="IC404" pad="1"/>
</signal>
<signal name="AOFI">
<contactref element="IC101" pad="10"/>
<contactref element="IC404" pad="5"/>
</signal>
<signal name="!ENC_CLICK">
<contactref element="IC101" pad="19"/>
<contactref element="SW401" pad="D"/>
</signal>
<signal name="HOTEND1">
<contactref element="IC101" pad="20"/>
<contactref element="R514" pad="1"/>
<contactref element="R513" pad="2"/>
</signal>
<signal name="Y-STEP">
<contactref element="IC101" pad="25"/>
<contactref element="X203" pad="STEP"/>
</signal>
<signal name="Y-DIR">
<contactref element="IC101" pad="26"/>
<contactref element="X203" pad="DIR"/>
</signal>
<signal name="!STEP-ENABLE">
<contactref element="IC101" pad="15"/>
<contactref element="X202" pad="!EN"/>
<contactref element="X203" pad="!EN"/>
<contactref element="X204" pad="!EN"/>
<contactref element="X201" pad="!EN"/>
<contactref element="X205" pad="!EN"/>
<contactref element="R103" pad="2"/>
<contactref element="R517" pad="1"/>
</signal>
<signal name="HOTBED">
<contactref element="IC101" pad="13"/>
<contactref element="R503" pad="1"/>
<contactref element="R502" pad="2"/>
</signal>
<signal name="HOTEND0">
<contactref element="IC101" pad="14"/>
<contactref element="R510" pad="1"/>
<contactref element="R509" pad="2"/>
</signal>
<signal name="X-STOP">
<contactref element="IC101" pad="21"/>
<contactref element="JP102" pad="1"/>
<contactref element="R301" pad="2"/>
</signal>
<signal name="Y-STOP">
<contactref element="IC101" pad="22"/>
<contactref element="JP102" pad="5"/>
<contactref element="R302" pad="2"/>
</signal>
<signal name="Z-STOP">
<contactref element="IC101" pad="23"/>
<contactref element="JP102" pad="3"/>
<contactref element="R303" pad="2"/>
</signal>
<signal name="X-STEP">
<contactref element="IC101" pad="16"/>
<contactref element="X202" pad="STEP"/>
</signal>
<signal name="X-DIR">
<contactref element="IC101" pad="24"/>
<contactref element="JP102" pad="9"/>
<contactref element="X202" pad="DIR"/>
</signal>
<signal name="Z-STEP">
<contactref element="IC101" pad="43"/>
<contactref element="X201" pad="STEP"/>
</signal>
<signal name="Z-DIR">
<contactref element="IC101" pad="42"/>
<contactref element="X201" pad="DIR"/>
</signal>
<signal name="E0-STEP">
<contactref element="IC101" pad="41"/>
<contactref element="X204" pad="STEP"/>
</signal>
<signal name="E0-DIR">
<contactref element="IC101" pad="40"/>
<contactref element="X204" pad="DIR"/>
</signal>
<signal name="E-THERM1">
<contactref element="IC101" pad="32"/>
<contactref element="R305" pad="2"/>
<contactref element="C305" pad="2"/>
<contactref element="JP305" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="IC101" pad="29"/>
<contactref element="R101" pad="1"/>
<contactref element="C107" pad="2"/>
<contactref element="C105" pad="+"/>
</signal>
<signal name="N$34">
<contactref element="IC101" pad="7"/>
<contactref element="C102" pad="2"/>
<contactref element="XTAL101" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="IC101" pad="8"/>
<contactref element="C104" pad="1"/>
<contactref element="XTAL101" pad="1"/>
</signal>
<signal name="X-RESETSLEEP">
<contactref element="X202" pad="!RST"/>
<contactref element="X202" pad="!SLP"/>
</signal>
<signal name="Y-RESETSLEEP">
<contactref element="X203" pad="!RST"/>
<contactref element="X203" pad="!SLP"/>
</signal>
<signal name="Z-RESETSLEEP">
<contactref element="X201" pad="!RST"/>
<contactref element="X201" pad="!SLP"/>
</signal>
<signal name="X-MS2">
<contactref element="X202" pad="MS2"/>
<contactref element="JP201" pad="3"/>
</signal>
<signal name="X-MOT-2B">
<contactref element="X202" pad="2B"/>
<contactref element="JP205" pad="1"/>
</signal>
<signal name="X-MOT-2A">
<contactref element="X202" pad="2A"/>
<contactref element="JP205" pad="2"/>
</signal>
<signal name="X-MOT-1A">
<contactref element="X202" pad="1A"/>
<contactref element="JP205" pad="3"/>
</signal>
<signal name="X-MOT-1B">
<contactref element="X202" pad="1B"/>
<contactref element="JP205" pad="4"/>
</signal>
<signal name="Y-MOT-2B">
<contactref element="X203" pad="2B"/>
<contactref element="JP206" pad="1"/>
</signal>
<signal name="Y-MOT-2A">
<contactref element="X203" pad="2A"/>
<contactref element="JP206" pad="2"/>
</signal>
<signal name="Y-MOT-1A">
<contactref element="X203" pad="1A"/>
<contactref element="JP206" pad="3"/>
</signal>
<signal name="Y-MOT-1B">
<contactref element="X203" pad="1B"/>
<contactref element="JP206" pad="4"/>
</signal>
<signal name="E-RESETSLEEP">
<contactref element="X204" pad="!RST"/>
<contactref element="X204" pad="!SLP"/>
</signal>
<signal name="E-MOT-2B">
<contactref element="X204" pad="2B"/>
<contactref element="JP210" pad="1"/>
</signal>
<signal name="E-MOT-2A">
<contactref element="X204" pad="2A"/>
<contactref element="JP210" pad="2"/>
</signal>
<signal name="E-MOT-1A">
<contactref element="X204" pad="1A"/>
<contactref element="JP210" pad="3"/>
</signal>
<signal name="E-MOT-1B">
<contactref element="X204" pad="1B"/>
<contactref element="JP210" pad="4"/>
</signal>
<signal name="X-MS3">
<contactref element="X202" pad="MS3"/>
<contactref element="JP201" pad="1"/>
</signal>
<signal name="Y-MS1">
<contactref element="X203" pad="MS1"/>
<contactref element="JP202" pad="5"/>
<contactref element="R202" pad="1"/>
</signal>
<signal name="Z-MS2">
<contactref element="X201" pad="MS2"/>
<contactref element="JP203" pad="3"/>
</signal>
<signal name="Z-MS3">
<contactref element="X201" pad="MS3"/>
<contactref element="JP203" pad="1"/>
</signal>
<signal name="E-MS1">
<contactref element="X204" pad="MS1"/>
<contactref element="JP208" pad="5"/>
<contactref element="R204" pad="1"/>
</signal>
<signal name="E-MS2">
<contactref element="X204" pad="MS2"/>
<contactref element="JP208" pad="3"/>
</signal>
<signal name="E-MS3">
<contactref element="X204" pad="MS3"/>
<contactref element="JP208" pad="1"/>
</signal>
<signal name="Y-MS2">
<contactref element="X203" pad="MS2"/>
<contactref element="JP202" pad="3"/>
</signal>
<signal name="Y-MS3">
<contactref element="X203" pad="MS3"/>
<contactref element="JP202" pad="1"/>
</signal>
<signal name="Z-MS1">
<contactref element="X201" pad="MS1"/>
<contactref element="JP203" pad="5"/>
<contactref element="R203" pad="1"/>
</signal>
<signal name="X-MS1">
<contactref element="X202" pad="MS1"/>
<contactref element="JP201" pad="5"/>
<contactref element="R201" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="X201" pad="1A"/>
<contactref element="JP204" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="JP204" pad="4"/>
<contactref element="JP207" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="JP207" pad="4"/>
<contactref element="X201" pad="1B"/>
</signal>
<signal name="N$22">
<contactref element="X201" pad="2A"/>
<contactref element="JP204" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="JP204" pad="1"/>
<contactref element="JP207" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="JP207" pad="1"/>
<contactref element="X201" pad="2B"/>
</signal>
<signal name="E-RESETSLEEP1">
<contactref element="X205" pad="!RST"/>
<contactref element="X205" pad="!SLP"/>
</signal>
<signal name="E-MOT-2B1">
<contactref element="X205" pad="2B"/>
<contactref element="JP211" pad="1"/>
</signal>
<signal name="E-MOT-2A1">
<contactref element="X205" pad="2A"/>
<contactref element="JP211" pad="2"/>
</signal>
<signal name="E-MOT-1A1">
<contactref element="X205" pad="1A"/>
<contactref element="JP211" pad="3"/>
</signal>
<signal name="E-MOT-1B1">
<contactref element="X205" pad="1B"/>
<contactref element="JP211" pad="4"/>
</signal>
<signal name="E-MS4">
<contactref element="X205" pad="MS1"/>
<contactref element="JP209" pad="5"/>
<contactref element="R205" pad="1"/>
</signal>
<signal name="E-MS5">
<contactref element="X205" pad="MS2"/>
<contactref element="JP209" pad="3"/>
</signal>
<signal name="E-MS6">
<contactref element="X205" pad="MS3"/>
<contactref element="JP209" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP301" pad="1"/>
<contactref element="R301" pad="1"/>
<contactref element="C301" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R303" pad="1"/>
<contactref element="JP303" pad="1"/>
<contactref element="C303" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="R302" pad="1"/>
<contactref element="JP302" pad="1"/>
<contactref element="C302" pad="2"/>
</signal>
<signal name="CAP1N">
<contactref element="C414" pad="2"/>
<contactref element="LCD401" pad="30"/>
<contactref element="C420" pad="2"/>
<contactref element="X403" pad="17"/>
</signal>
<signal name="CAP1P">
<contactref element="C414" pad="1"/>
<contactref element="LCD401" pad="29"/>
<contactref element="X403" pad="18"/>
</signal>
<signal name="CAP2P">
<contactref element="LCD401" pad="28"/>
<contactref element="C416" pad="1"/>
<contactref element="X403" pad="19"/>
</signal>
<signal name="CAP2N">
<contactref element="C416" pad="2"/>
<contactref element="LCD401" pad="27"/>
<contactref element="X403" pad="20"/>
</signal>
<signal name="CAP3P">
<contactref element="LCD401" pad="31"/>
<contactref element="C420" pad="1"/>
<contactref element="X403" pad="16"/>
</signal>
<signal name="VOUT">
<contactref element="LCD401" pad="32"/>
<contactref element="C421" pad="1"/>
<contactref element="X403" pad="15"/>
</signal>
<signal name="V4">
<contactref element="LCD401" pad="25"/>
<contactref element="C422" pad="1"/>
<contactref element="X403" pad="23"/>
</signal>
<signal name="V3">
<contactref element="LCD401" pad="24"/>
<contactref element="C423" pad="1"/>
<contactref element="X403" pad="24"/>
</signal>
<signal name="V2">
<contactref element="LCD401" pad="23"/>
<contactref element="C424" pad="1"/>
<contactref element="X403" pad="25"/>
</signal>
<signal name="V1">
<contactref element="LCD401" pad="22"/>
<contactref element="C425" pad="1"/>
<contactref element="X403" pad="26"/>
</signal>
<signal name="V0">
<contactref element="LCD401" pad="21"/>
<contactref element="C426" pad="1"/>
<contactref element="X403" pad="27"/>
</signal>
<signal name="LCD_C3">
<contactref element="R408" pad="1"/>
<contactref element="LCD401" pad="20"/>
</signal>
<signal name="LCD_C1">
<contactref element="R410" pad="1"/>
<contactref element="LCD401" pad="18"/>
</signal>
<signal name="LCD_C2">
<contactref element="R409" pad="1"/>
<contactref element="LCD401" pad="19"/>
</signal>
<signal name="+3V3">
<contactref element="C417" pad="2"/>
<contactref element="LCD401" pad="34"/>
<contactref element="LCD401" pad="35"/>
<contactref element="C413" pad="1"/>
<contactref element="C412" pad="+"/>
<contactref element="R407" pad="1"/>
<contactref element="IC403" pad="4"/>
<contactref element="C407" pad="+"/>
<contactref element="C405" pad="2"/>
<contactref element="R411" pad="1"/>
<contactref element="X402" pad="4"/>
<contactref element="C401" pad="2"/>
<contactref element="IC401" pad="1"/>
<contactref element="X403" pad="22"/>
</signal>
<signal name="MOSI">
<contactref element="LCD401" pad="36"/>
<contactref element="X402" pad="3"/>
<contactref element="IC401" pad="2"/>
<contactref element="X403" pad="13"/>
</signal>
<signal name="MISO">
<contactref element="X402" pad="7"/>
<contactref element="IC401" pad="7"/>
</signal>
<signal name="SCK">
<contactref element="LCD401" pad="37"/>
<contactref element="X402" pad="5"/>
<contactref element="IC401" pad="10"/>
<contactref element="X403" pad="12"/>
</signal>
<signal name="!ENB_LCD">
<contactref element="LCD401" pad="40"/>
<contactref element="IC401" pad="4"/>
<contactref element="X403" pad="1"/>
</signal>
<signal name="A0_LCD">
<contactref element="LCD401" pad="38"/>
<contactref element="IC401" pad="12"/>
<contactref element="X403" pad="3"/>
</signal>
<signal name="!ENB_SD">
<contactref element="X402" pad="2"/>
<contactref element="IC401" pad="15"/>
</signal>
<signal name="N$15">
<contactref element="R401" pad="2"/>
<contactref element="IC401" pad="6"/>
</signal>
<signal name="!LCD_RST">
<contactref element="LCD401" pad="39"/>
<contactref element="R407" pad="2"/>
<contactref element="C411" pad="2"/>
<contactref element="X403" pad="2"/>
</signal>
<signal name="USBDP">
<contactref element="IC404" pad="15"/>
<contactref element="X401" pad="3"/>
<contactref element="IC402" pad="3"/>
</signal>
<signal name="USBDM">
<contactref element="IC404" pad="16"/>
<contactref element="X401" pad="2"/>
<contactref element="IC402" pad="5"/>
</signal>
<signal name="3V3">
<contactref element="C404" pad="2"/>
<contactref element="IC404" pad="17"/>
</signal>
<signal name="N$4">
<contactref element="R402" pad="1"/>
<contactref element="X401" pad="6"/>
<contactref element="X401" pad="7"/>
<contactref element="X401" pad="8"/>
<contactref element="X401" pad="9"/>
<contactref element="X401" pad="10"/>
<contactref element="X401" pad="11"/>
</signal>
<signal name="N$6">
<contactref element="LED402" pad="A"/>
<contactref element="R405" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED403" pad="A"/>
<contactref element="R406" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R404" pad="2"/>
<contactref element="R403" pad="1"/>
<contactref element="IC404" pad="19"/>
</signal>
<signal name="N$8">
<contactref element="IC402" pad="1"/>
<contactref element="R404" pad="1"/>
<contactref element="X401" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED402" pad="C"/>
<contactref element="IC404" pad="23"/>
</signal>
<signal name="N$3">
<contactref element="IC404" pad="22"/>
<contactref element="LED403" pad="C"/>
</signal>
<signal name="N$999">
<contactref element="R511" pad="1"/>
<contactref element="R510" pad="2"/>
<contactref element="T503" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="R504" pad="1"/>
<contactref element="R503" pad="2"/>
<contactref element="T502" pad="4"/>
</signal>
<signal name="N$31">
<contactref element="R507" pad="1"/>
<contactref element="C502" pad="2"/>
<contactref element="JP502" pad="1"/>
<contactref element="JP502" pad="2"/>
<contactref element="T502" pad="5"/>
<contactref element="T502" pad="6"/>
<contactref element="T502" pad="7"/>
<contactref element="T502" pad="8"/>
<contactref element="D502" pad="A"/>
</signal>
<signal name="N$43">
<contactref element="R505" pad="2"/>
<contactref element="R506" pad="1"/>
<contactref element="T501" pad="4"/>
</signal>
<signal name="N$44">
<contactref element="JP501" pad="2"/>
<contactref element="T501" pad="5"/>
<contactref element="T501" pad="8"/>
<contactref element="T501" pad="7"/>
<contactref element="T501" pad="6"/>
<contactref element="R501" pad="1"/>
<contactref element="C501" pad="2"/>
<contactref element="D501" pad="A"/>
</signal>
<signal name="N$49">
<contactref element="R515" pad="1"/>
<contactref element="R514" pad="2"/>
<contactref element="T504" pad="4"/>
</signal>
<signal name="LED1">
<contactref element="R606" pad="2"/>
<contactref element="LED602" pad="A"/>
</signal>
<signal name="+UB">
<contactref element="X602" pad="4"/>
<contactref element="X602" pad="3"/>
<contactref element="X601" pad="1"/>
<contactref element="X601" pad="2"/>
<contactref element="F601" pad="1"/>
<contactref element="F601" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="C611" pad="2"/>
<contactref element="C610" pad="2"/>
<contactref element="C609" pad="+"/>
<contactref element="L602" pad="2"/>
<contactref element="IC602" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="IC601" pad="1"/>
<contactref element="L601" pad="1"/>
<contactref element="D604" pad="C"/>
</signal>
<signal name="+24V">
<contactref element="C603" pad="2"/>
<contactref element="C601" pad="2"/>
<contactref element="IC601" pad="8"/>
<contactref element="C602" pad="1"/>
<contactref element="C604" pad="2"/>
<contactref element="D601" pad="P$1"/>
<contactref element="C207" pad="+"/>
<contactref element="C209" pad="2"/>
<contactref element="X202" pad="VMOT"/>
<contactref element="C217" pad="+"/>
<contactref element="C219" pad="2"/>
<contactref element="X204" pad="VMOT"/>
<contactref element="C218" pad="+"/>
<contactref element="C220" pad="2"/>
<contactref element="X205" pad="VMOT"/>
<contactref element="C208" pad="+"/>
<contactref element="C210" pad="2"/>
<contactref element="X203" pad="VMOT"/>
<contactref element="C211" pad="+"/>
<contactref element="C212" pad="2"/>
<contactref element="X201" pad="VMOT"/>
<contactref element="JP502" pad="3"/>
<contactref element="JP502" pad="4"/>
<contactref element="JP505" pad="2"/>
<contactref element="JP506" pad="2"/>
<contactref element="D502" pad="C"/>
<contactref element="D503" pad="C"/>
<contactref element="D504" pad="C"/>
<contactref element="F601" pad="2"/>
<contactref element="F601" pad="4"/>
</signal>
<signal name="N$46">
<contactref element="R603" pad="2"/>
<contactref element="R604" pad="1"/>
<contactref element="IC601" pad="5"/>
</signal>
<signal name="N$47">
<contactref element="IC601" pad="4"/>
<contactref element="C606" pad="2"/>
<contactref element="C605" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="C606" pad="1"/>
<contactref element="R601" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="LED401" pad="A"/>
<contactref element="R411" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="LED502" pad="A"/>
<contactref element="R508" pad="1"/>
</signal>
<signal name="N$56">
<contactref element="LED501" pad="A"/>
<contactref element="R502" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="LED503" pad="A"/>
<contactref element="R509" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="LED504" pad="A"/>
<contactref element="R513" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="LED101" pad="A"/>
<contactref element="R104" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="R104" pad="2"/>
<contactref element="T101" pad="C"/>
</signal>
<signal name="N$61">
<contactref element="T101" pad="B"/>
<contactref element="R103" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="JP507" pad="1"/>
<contactref element="T505" pad="3"/>
</signal>
<signal name="N$64">
<contactref element="R517" pad="2"/>
<contactref element="R518" pad="2"/>
<contactref element="T505" pad="1"/>
</signal>
<signal name="12V">
<contactref element="JP503" pad="1"/>
<contactref element="L601" pad="2"/>
<contactref element="R603" pad="1"/>
<contactref element="C607" pad="+"/>
<contactref element="C608" pad="2"/>
<contactref element="JP501" pad="1"/>
<contactref element="L602" pad="1"/>
<contactref element="D501" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="T503" pad="8"/>
<contactref element="T503" pad="7"/>
<contactref element="T503" pad="6"/>
<contactref element="R512" pad="1"/>
<contactref element="C503" pad="2"/>
<contactref element="T503" pad="5"/>
<contactref element="JP505" pad="1"/>
<contactref element="D503" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="JP506" pad="1"/>
<contactref element="T504" pad="5"/>
<contactref element="R516" pad="1"/>
<contactref element="C504" pad="2"/>
<contactref element="T504" pad="6"/>
<contactref element="T504" pad="7"/>
<contactref element="T504" pad="8"/>
<contactref element="D504" pad="A"/>
</signal>
<signal name="N$17">
</signal>
<signal name="N$26">
</signal>
<signal name="N$11">
<contactref element="X404" pad="2"/>
<contactref element="R412" pad="1"/>
</signal>
<signal name="VMOT">
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="X" pad="VMOT"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="22"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="X1" pad="VMOT"/>
<contactref element="C14" pad="2"/>
<contactref element="IC2" pad="28"/>
<contactref element="IC2" pad="22"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="X2" pad="VMOT"/>
<contactref element="C21" pad="2"/>
<contactref element="IC3" pad="28"/>
<contactref element="IC3" pad="22"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="X3" pad="VMOT"/>
<contactref element="C28" pad="2"/>
<contactref element="IC4" pad="28"/>
<contactref element="IC4" pad="22"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C33" pad="1"/>
<contactref element="X4" pad="VMOT"/>
<contactref element="C35" pad="2"/>
<contactref element="IC5" pad="28"/>
<contactref element="IC5" pad="22"/>
<contactref element="C36" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C40" pad="1"/>
<contactref element="X5" pad="VMOT"/>
<contactref element="C42" pad="2"/>
<contactref element="IC6" pad="28"/>
<contactref element="IC6" pad="22"/>
</signal>
<signal name="VDD">
<contactref element="C2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="X" pad="VDD"/>
<contactref element="IC1" pad="15"/>
<contactref element="C10" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="X1" pad="VDD"/>
<contactref element="IC2" pad="15"/>
<contactref element="C17" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="X2" pad="VDD"/>
<contactref element="IC3" pad="15"/>
<contactref element="C24" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="X3" pad="VDD"/>
<contactref element="IC4" pad="15"/>
<contactref element="C31" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="X4" pad="VDD"/>
<contactref element="IC5" pad="15"/>
<contactref element="C38" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="R39" pad="2"/>
<contactref element="X5" pad="VDD"/>
<contactref element="IC6" pad="15"/>
<contactref element="C43" pad="2"/>
<contactref element="R43" pad="1"/>
<contactref element="R44" pad="1"/>
<contactref element="T1" pad="3"/>
<contactref element="C44" pad="2"/>
<contactref element="R46" pad="1"/>
<contactref element="R47" pad="1"/>
<contactref element="T2" pad="3"/>
<contactref element="C45" pad="2"/>
<contactref element="R49" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="XOUT2B">
<contactref element="X" pad="2B"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="XOUT2A">
<contactref element="X" pad="2A"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="XOUT1A">
<contactref element="X" pad="1A"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="XOUT1B">
<contactref element="X" pad="1B"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="XENABLE">
<contactref element="R6" pad="2"/>
<contactref element="X" pad="!EN"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="XMS1">
<contactref element="X" pad="MS1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="XMS2">
<contactref element="X" pad="MS2"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="XMS3">
<contactref element="X" pad="MS3"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="XRESET">
<contactref element="X" pad="!RST"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="XSLEEP">
<contactref element="R7" pad="2"/>
<contactref element="X" pad="!SLP"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="XSTEP">
<contactref element="X" pad="STEP"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="XDIR">
<contactref element="X" pad="DIR"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="XSENSE2">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="XSENSE1">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="XCP1">
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="XCP2">
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="XVCP">
<contactref element="C6" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="XROSC">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="XVREG">
<contactref element="C7" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="XREF">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="17"/>
<contactref element="R4" pad="1"/>
<contactref element="R4" pad="3"/>
</signal>
<signal name="XOUT2B1">
<contactref element="X1" pad="2B"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="XOUT2A1">
<contactref element="X1" pad="2A"/>
<contactref element="IC2" pad="26"/>
</signal>
<signal name="XOUT1A1">
<contactref element="X1" pad="1A"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="XOUT1B1">
<contactref element="X1" pad="1B"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="XENABLE1">
<contactref element="R9" pad="2"/>
<contactref element="X1" pad="!EN"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="XMS4">
<contactref element="X1" pad="MS1"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="XMS5">
<contactref element="X1" pad="MS2"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="XMS6">
<contactref element="X1" pad="MS3"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="XRESET1">
<contactref element="X1" pad="!RST"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="XSLEEP1">
<contactref element="R10" pad="2"/>
<contactref element="X1" pad="!SLP"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="XSTEP1">
<contactref element="X1" pad="STEP"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="XDIR1">
<contactref element="X1" pad="DIR"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="XSENSE3">
<contactref element="R12" pad="2"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="XSENSE4">
<contactref element="R13" pad="1"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="XCP3">
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="XCP4">
<contactref element="C11" pad="1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="XVCP1">
<contactref element="C12" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="XROSC1">
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="XVREG1">
<contactref element="C13" pad="1"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="XREF1">
<contactref element="R11" pad="1"/>
<contactref element="IC2" pad="17"/>
<contactref element="R14" pad="1"/>
<contactref element="R14" pad="3"/>
</signal>
<signal name="XOUT2B2">
<contactref element="X2" pad="2B"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="XOUT2A2">
<contactref element="X2" pad="2A"/>
<contactref element="IC3" pad="26"/>
</signal>
<signal name="XOUT1A2">
<contactref element="X2" pad="1A"/>
<contactref element="IC3" pad="24"/>
</signal>
<signal name="XOUT1B2">
<contactref element="X2" pad="1B"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="XENABLE2">
<contactref element="R16" pad="2"/>
<contactref element="X2" pad="!EN"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="XMS7">
<contactref element="X2" pad="MS1"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="XMS8">
<contactref element="X2" pad="MS2"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="XMS9">
<contactref element="X2" pad="MS3"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="XRESET2">
<contactref element="X2" pad="!RST"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="XSLEEP2">
<contactref element="R17" pad="2"/>
<contactref element="X2" pad="!SLP"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="XSTEP2">
<contactref element="X2" pad="STEP"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="XDIR2">
<contactref element="X2" pad="DIR"/>
<contactref element="IC3" pad="19"/>
</signal>
<signal name="XSENSE5">
<contactref element="R19" pad="2"/>
<contactref element="IC3" pad="27"/>
</signal>
<signal name="XSENSE6">
<contactref element="R20" pad="1"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="XCP5">
<contactref element="C18" pad="2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="XCP6">
<contactref element="C18" pad="1"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="XVCP2">
<contactref element="C19" pad="2"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="XROSC2">
<contactref element="R15" pad="2"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="XVREG2">
<contactref element="C20" pad="1"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="XREF2">
<contactref element="R18" pad="1"/>
<contactref element="IC3" pad="17"/>
<contactref element="R21" pad="1"/>
<contactref element="R21" pad="3"/>
</signal>
<signal name="XOUT2B3">
<contactref element="X3" pad="2B"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="XOUT2A3">
<contactref element="X3" pad="2A"/>
<contactref element="IC4" pad="26"/>
</signal>
<signal name="XOUT1A3">
<contactref element="X3" pad="1A"/>
<contactref element="IC4" pad="24"/>
</signal>
<signal name="XOUT1B3">
<contactref element="X3" pad="1B"/>
<contactref element="IC4" pad="21"/>
</signal>
<signal name="XENABLE3">
<contactref element="R23" pad="2"/>
<contactref element="X3" pad="!EN"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="XMS10">
<contactref element="X3" pad="MS1"/>
<contactref element="IC4" pad="9"/>
</signal>
<signal name="XMS11">
<contactref element="X3" pad="MS2"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="XMS12">
<contactref element="X3" pad="MS3"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="XRESET3">
<contactref element="X3" pad="!RST"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="XSLEEP3">
<contactref element="R24" pad="2"/>
<contactref element="X3" pad="!SLP"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="XSTEP3">
<contactref element="X3" pad="STEP"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="XDIR3">
<contactref element="X3" pad="DIR"/>
<contactref element="IC4" pad="19"/>
</signal>
<signal name="XSENSE7">
<contactref element="R26" pad="2"/>
<contactref element="IC4" pad="27"/>
</signal>
<signal name="XSENSE8">
<contactref element="R27" pad="1"/>
<contactref element="IC4" pad="23"/>
</signal>
<signal name="XCP7">
<contactref element="C25" pad="2"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="XCP8">
<contactref element="C25" pad="1"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="XVCP3">
<contactref element="C26" pad="2"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="XROSC3">
<contactref element="R22" pad="2"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="XVREG3">
<contactref element="C27" pad="1"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="XREF3">
<contactref element="R25" pad="1"/>
<contactref element="IC4" pad="17"/>
<contactref element="R28" pad="1"/>
<contactref element="R28" pad="3"/>
</signal>
<signal name="XOUT2B4">
<contactref element="X4" pad="2B"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="XOUT2A4">
<contactref element="X4" pad="2A"/>
<contactref element="IC5" pad="26"/>
</signal>
<signal name="XOUT1A4">
<contactref element="X4" pad="1A"/>
<contactref element="IC5" pad="24"/>
</signal>
<signal name="XOUT1B4">
<contactref element="X4" pad="1B"/>
<contactref element="IC5" pad="21"/>
</signal>
<signal name="XENABLE4">
<contactref element="R30" pad="2"/>
<contactref element="X4" pad="!EN"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="XMS13">
<contactref element="X4" pad="MS1"/>
<contactref element="IC5" pad="9"/>
</signal>
<signal name="XMS14">
<contactref element="X4" pad="MS2"/>
<contactref element="IC5" pad="10"/>
</signal>
<signal name="XMS15">
<contactref element="X4" pad="MS3"/>
<contactref element="IC5" pad="11"/>
</signal>
<signal name="XRESET4">
<contactref element="X4" pad="!RST"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="XSLEEP4">
<contactref element="R31" pad="2"/>
<contactref element="X4" pad="!SLP"/>
<contactref element="IC5" pad="14"/>
</signal>
<signal name="XSTEP4">
<contactref element="X4" pad="STEP"/>
<contactref element="IC5" pad="16"/>
</signal>
<signal name="XDIR4">
<contactref element="X4" pad="DIR"/>
<contactref element="IC5" pad="19"/>
</signal>
<signal name="XSENSE9">
<contactref element="R33" pad="2"/>
<contactref element="IC5" pad="27"/>
</signal>
<signal name="XSENSE10">
<contactref element="R34" pad="1"/>
<contactref element="IC5" pad="23"/>
</signal>
<signal name="XCP9">
<contactref element="C32" pad="2"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="XCP10">
<contactref element="C32" pad="1"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="XVCP4">
<contactref element="C33" pad="2"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="XROSC4">
<contactref element="R29" pad="2"/>
<contactref element="IC5" pad="13"/>
</signal>
<signal name="XVREG4">
<contactref element="C34" pad="1"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="XREF4">
<contactref element="R32" pad="1"/>
<contactref element="IC5" pad="17"/>
<contactref element="R35" pad="1"/>
<contactref element="R35" pad="3"/>
</signal>
<signal name="XOUT2B5">
<contactref element="X5" pad="2B"/>
<contactref element="IC6" pad="1"/>
</signal>
<signal name="XOUT2A5">
<contactref element="X5" pad="2A"/>
<contactref element="IC6" pad="26"/>
</signal>
<signal name="XOUT1A5">
<contactref element="X5" pad="1A"/>
<contactref element="IC6" pad="24"/>
</signal>
<signal name="XOUT1B5">
<contactref element="X5" pad="1B"/>
<contactref element="IC6" pad="21"/>
</signal>
<signal name="XENABLE5">
<contactref element="R37" pad="2"/>
<contactref element="X5" pad="!EN"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="XMS16">
<contactref element="X5" pad="MS1"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="XMS17">
<contactref element="X5" pad="MS2"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="XMS18">
<contactref element="X5" pad="MS3"/>
<contactref element="IC6" pad="11"/>
</signal>
<signal name="XRESET5">
<contactref element="X5" pad="!RST"/>
<contactref element="IC6" pad="12"/>
</signal>
<signal name="XSLEEP5">
<contactref element="R38" pad="2"/>
<contactref element="X5" pad="!SLP"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="XSTEP5">
<contactref element="X5" pad="STEP"/>
<contactref element="IC6" pad="16"/>
</signal>
<signal name="XDIR5">
<contactref element="X5" pad="DIR"/>
<contactref element="IC6" pad="19"/>
</signal>
<signal name="XSENSE11">
<contactref element="R40" pad="2"/>
<contactref element="IC6" pad="27"/>
</signal>
<signal name="XSENSE12">
<contactref element="R41" pad="1"/>
<contactref element="IC6" pad="23"/>
</signal>
<signal name="XCP11">
<contactref element="C39" pad="2"/>
<contactref element="IC6" pad="4"/>
</signal>
<signal name="XCP12">
<contactref element="C39" pad="1"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="XVCP5">
<contactref element="C40" pad="2"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="XROSC5">
<contactref element="R36" pad="2"/>
<contactref element="IC6" pad="13"/>
</signal>
<signal name="XVREG5">
<contactref element="C41" pad="1"/>
<contactref element="IC6" pad="8"/>
</signal>
<signal name="XREF5">
<contactref element="R39" pad="1"/>
<contactref element="IC6" pad="17"/>
<contactref element="R42" pad="1"/>
<contactref element="R42" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R43" pad="2"/>
<contactref element="X6" pad="A"/>
</signal>
<signal name="OUT">
<contactref element="R44" pad="2"/>
<contactref element="X6" pad="CO"/>
<contactref element="T1" pad="1"/>
<contactref element="R47" pad="2"/>
<contactref element="X7" pad="CO"/>
<contactref element="T2" pad="1"/>
<contactref element="R50" pad="2"/>
<contactref element="X8" pad="CO"/>
<contactref element="T3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R45" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="T1" pad="2"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R46" pad="2"/>
<contactref element="X7" pad="A"/>
</signal>
<signal name="N$27">
<contactref element="R48" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="T2" pad="2"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R49" pad="2"/>
<contactref element="X8" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="R51" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$38">
<contactref element="T3" pad="2"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R511" pad="2"/>
<contactref element="T503" pad="1"/>
<contactref element="T503" pad="2"/>
<contactref element="T503" pad="3"/>
<contactref element="R512" pad="2"/>
<contactref element="C503" pad="1"/>
<contactref element="R515" pad="2"/>
<contactref element="T504" pad="1"/>
<contactref element="T504" pad="2"/>
<contactref element="T504" pad="3"/>
<contactref element="R516" pad="2"/>
<contactref element="C504" pad="1"/>
<contactref element="LED503" pad="C"/>
<contactref element="LED504" pad="C"/>
<contactref element="F501" pad="2"/>
<contactref element="F501" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
